Rabid prototypes Tau bootloader flashed to use Arduino interface, but could not program.

Flashing through Microchip studio directly instead, so no bootloader required.

Port definitions

C:\Program Files (x86)\Atmel\Studio\7.0\packs\atmel\SAMD21\_DFP\1.3.395\samd21a\include\instance

PORT at 0x41004400

A screenshot of a computer

Description automatically generated with medium confidence

https://forum.digikey.com/t/getting-started-with-the-sam-d21-xplained-pro-without-asf/13176

Graphical user interface, text

Description automatically generated

Table

Description automatically generated

<https://cboard.cprogramming.com/windows-programming/3144-moving-mouse-pointer.html>

<https://stackoverflow.com/questions/16955806/how-to-add-c-and-h-files-to-atmel-studio-6>

C:\msys64\mingw64\x86\_64-w64-mingw32\include

https://asf.microchip.com/docs/latest/saml21/html/udi\_hid\_mouse\_quickstart.html

https://asf.microchip.com/docs/latest/saml21/html/group\_\_udi\_\_hid\_\_mouse\_\_group.html

Table

Description automatically generated with medium confidence